**PCGI Panelling Preventive and Periodical Checks & Maintenance during CAMC Period (6th, 7th, 8th, 9th & 10th year) at Quarterly interval for every year from 6th to 10th year:**

***Note: The Unconditional Warranty is applicable as per Agreement - Section-IV - General Conditions of Contract – Clause:15.***

**1. Visual Inspection:**

- Check the overall condition of the panelling for any signs of corrosion.

- Examine the seams and joints for gaps or separation.

**2. Sealant Inspection:**

- Inspect any sealants or caulking around panel edges, joints, or penetrations for signs of deterioration or cracking.

- Replace any damaged or deteriorated sealants to maintain weatherproofing and prevent water infiltration.

**3. Hardware Inspection:**

- Check the condition of any hardware components, such as screws, bolts, or brackets, for signs of rust or corrosion.

- Tighten loose hardware and replace any corroded components as needed to ensure structural integrity.

**4. Coving Inspection:**

- Check the condition of 2D & 3D coving for any damage or signs of corrosion.

- Replace if found damaged with new one.