|  |  |
| --- | --- |
| To, | Date: 28-12- 2023 |
| The Executive Engineer, | **Furniture** .Pro- D-Tech /572 /2023-24 |
| (Engineer In-charge) | Validity – 90 Days |
| TSMSIDC, Hyderabad Division. | GST No:- 36APFPK9302P1ZG |
| GST NO:- | Bagya Laxmi Colony |
| Mail ID:- | Subash Nagar IDA Jeedimetla |
| Mob No:- | Proprietor Code 4687569 |

**QUOTATION**

Sub: Our quotation for SOTC Gandhi Hospital, 8th floor, Secunderabad.

Ref: your enquiry dated 11-12-2023.

Dear Sir,

We are pleased to submit our quotation for SOTC Gandhi. The enclosed prices cover a 5-year warranty, and CAMC prices for the 6th to 10th year are presented separately for your convenience.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S. No** | **Particulars** | **Qty** | **Unit Rate** | **Total** |
| 1 | Monitor stand beside beds in ICU’s & TIR’s | **31** | 5,692/- | **1,76,452.00** |
| 2 | Double arm Surgical Pendant (supported): The pendant shall be imparted & comply with NFPA99c/HTM 02 - 01/ISO7396 -1/DIN. The support arms shall be extremely robust and revolve on high quality bearings so that pendant head glides smoothly and quickly to any desired position. double moveable arms with total coverage of not less than 1800mm and 330deg, horizontal movement for each arm, which can be easily adjusted to suit desired mode of operation. Vertical movement shall be motorized. Weight carrying capacity of the arm shall not be less than 180 kgs Shall have pneumatic brakes The pendant service heads shall be modular with minimum 1200mm head. the head shall be capable of accepting a range of shavasana infusion poles or other accessories. The pendant heads shall support the range of physiological Monitor Mounting solutions. Shall be dual art of 800mm/8tXfmm.05 no’s platforms of not less than 5tXlmm x5tXbnm x400mm,01 no’s Drawer for place Accessories. Each platform shall have a weight bearing capacity of minimum 30kg each. Sail has iv rod stand with capacity of 30 kg with 4-hooks for each rod. medical gas outlets CO2-02 NOS, Vacuum - 2n0s, Air (7bar)-2nos, Electrical sockets12no, shall provide on the service head (6on each side), DAT port RJ-45/cat6 -2nos. all interface for integration, braking systems, a small spring arm on the side support an additional monitor. | **6** | 1300000 | **78,00,000.00** |
|  |  |  | Total | **79,76,452.00** |
| GST @18% | | | | **14,35,761.00 14,35,761.00** |
| Total without CAMC | | | | **94,12,213.00** |
| CAMC Amount | | | | **35,89,405.00** |
| Total including CAMC | | | | **1,30,01,618** |

**(Rupees: -(One Crore Thirty Lakhs One Thousand Six Hundred and Eighteen only)**

Comprehensive Annual Maintanance Charges post warranty period for 5 years(6th to 10th year) @9, 9, 9, 9, 9 % respectively.

|  |  |  |  |
| --- | --- | --- | --- |
| Base Price | | | **79,76,452** |
| S.No | Year | CAMC % | Amount |
| 1 | 6th | 9 | 7,17,881 |
| 2 | 7th | 9 | 7,17,881 |
| 3 | 8th | 9 | 7,17,881 |
| 4 | 9th | 9 | 7,17,881 |
| 5 | 10th | 9 | 7,17,881 |
| Total % | | 45 |  |
| Total Amount | | | **35,89,405** |

**TERMS & CONDITIONS: -**

1. Packing, Forwarding & Transportation Charges: - **Included**

2. GST: - **Applicable as mentioned above.**

3. Payment: - **As per norms.**

4. Delivery: - 1 to 2 Weeks confirmed order.

**A close-up of a logo

Description automatically generated**

K.Venkatesh

+919989776972